Figure 2: Position shifts required to fill out the gaps between taps. The empirically determined correction is shown as the thin line. Also shown, offset for clarity, are the current CALDB implementation of the degap correction (red pluses; shifted upwards), and a 5^{th}-order polynomial fit to the empirical solution (blue diamonds; shifted downwards). Note the large difference between the CALDB and empirical solutions for tap 112.